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	Engine, drive system and battery

	Drive system
	
	4x4 (AWD)

	E-Machine(s)
	Type
	PSM/PSM

	Rated power (peak) (electric)
	kW
	360

	Rated torque (peak) (electric)
	Nm
	800

	Battery type
	
	Lithium-ion

	recuperation power max.
	kW
	Up to 300

	AC charging power, max. (standard/optional)
	kW
	11/22

	DC charging power, max.
	kW
	330

	DC charging time 10%-80% SOC (net)[endnoteRef:1] [1:  The charging times correspond to a 10-80 % charge when using a DC fast charging station in the "K" or "L" category in accordance with EN17186 with a charging current of 500 A.] 

	min
	22

	Recharged range in 10 minutes max[endnoteRef:2] [2:  The specified recharged range (WLTP) after 10 minutes was determined using the maximum DC charging power in accordance with ISO/SAE 12906 under the conditions described therein.] 

	km
	325

	Dimensions and weights

	Wheelbase
	mm
	2,962

	Track width, front/rear
	mm
	1,641/1,620 

	Length/width/height
	mm
	4,883/1,892/1,503

	Turning circle
	m
	12.10

	Luggage compartment capacity, VDA[endnoteRef:3] [3:  according to Directive ISO 3832:2002-06. Boot capacity may differ depending on special equipment.] 

	litre
	470

	Volume Frunk (liquid)[endnoteRef:4] [4:  According to Directive ISO 3832:2002-06.] 

	litre
	101

	Kerb weight[endnoteRef:5] [5:  Kerb weight, ready-to-drive in accordance with EU.] 

	kg
	2,460

	payload
	kg
	505

	permissible gross mass
	kg
	2,965

	Driving performance, consumption and range

	Acceleration 0 - 100 km/h
	s
	4.0

	Top speed
	km/h
	210

	Energy consumption (combined)[endnoteRef:6]  [6:  The specified values were determined in accordance with the prescribed measurement procedure WLTP (Worldwide harmonized Light-duty vehicles Test 
Procedures). The energy consumption and CO2 emissions of a passenger car depend not only on the efficient utilisation of fuel or the respective energy 
carrier by the car, but also on the driving style and other non-technical factors.] 

	kWh/100 km
	18.5 – 14.1

	CO₂ emissions (combined)6
	g/km
	0

	Electric range6
	km
	592 - 762

	CO2-Class6
	
	A



image1.emf

image2.emf

